
Release1.0.0.4(MII)
=======================================================================

1. Test with the two same configuration of Intel machines.
2. Arrange one as receive and another to transfer the data.
3. Place the devices facing each other.
4. The application is command based.
5. Use the command ./serialIrDA --help from the location /Application (cd /Applications) for application commands.
6. Take only MCS7780 device to test on the both sides like to send and receive.

Note: This is release is only for Intel MacOSX10.4.x

